1. Obtain the obstacle and mission waypoints from interop
2. Convert them all into universal transverse Mercator
3. Check for obstacle between two waypoints
4. Perform avoidance path planning
5. Optimize the output of path planning
6. Convert back into GPS
7. Write into waypoints file